CITY OF DETROIT

SPECIAL PROVISION FOR

**OVERLAY COLD PLASTIC PAVEMENT MARKING MATERIAL**

# SGJJR:ESM 1 of 1 01-24-17

1. **Description.** This work consists of providing and applying cold plastic permanent pavement markings in accordance with the Michigan Manual of Uniform Traffic Control Devices. Provide markings, shapes, spacing and dimensions as shown on plans.
2. **Materials.** Select pavement marking material from the Qualified Products List (QPL) in accordance with section 920 of the Michigan Department of Transportation Standard Specifications for Construction.
3. **Construction.** Place permanent pavement markings in accordance with section 811 of the Michigan Department of Transportation Standard Specifications for Construction.
4. **Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

\_Pavt Mrkg, Ovly Cold Plastic, Chevron Sym ...............................................................Each

\_Pavt Mrkg, Ovly Cold Plastic, Yield Sym ....................................................................Each

\_Pavt Mrkg, Ovly Cold Plastic, ADA Sym, Blue ............................................................Each

\_Pavt Mrkg, Ovly Cold Plastic, Loading Zone, Yellow ..................................................Each

**\_Pavt Mrkg, Ovly Cold Plastic, (symbol)** will be measured and paid for at the contract unit price per each unit installed. The unit price shall be payment in full for furnishing all labor, equipment and material to furnish and install pavement marking symbols as shown on the plans or as directed by the Engineer.