|  |  |  |
| --- | --- | --- |
|  | CITY OF DETROIT |  |
| SPECIAL PROVISION FOR  **QWICK KURB** |  |
| SGJJR:AMR | 1 of 2 | 01-24-17 |

1. **Description.** This work consists of furnishing and installing Qwick Kurbs as shown on the plans and as directed by the Engineer. Complete this work in accordance to the applicable sections of the standard specifications and this special provision. Follow industry standards and conform to the details as shown on the plans.
2. **Materials.** Furnish tools and equipment as recommended by the manufacturer and as approved by the Engineer. Use equipment and materials from a single manufacturer throughout the entire project.

Kurb Elements - The Qwick Kurb shall consist of type L60 mid curb sections with a length of 44 1/2” by 10 5/8” wide by 3 3/8” tall, type L61 end sections with a length of 21” by 9 5/8” wide by 3 3/8” tall, and L62 end sections with a length of 18 5/8” and width of 9 5/8” and a height of 3 3/8”.

Uprights – the uprights shall consist of type L125 with a white post, white base and green reflective sheeting

Warranty - Any bidder failing to provide the required Warranties of FHWA Acceptance letter will be disqualified.

Roadway Traffic Hazard Warranty - As a condition of this bid, Supplier must provide with the bid a manufacturer’s warranty against damage from all normal vehicular roadway traffic for the separator units, profile reflectors and asphalt mollies at 100% for the first two years, and at least 50% of the replacement value for three additional years.

Workmanship and Materials Warranty – As a condition of this bid, Supplier must provide with the bid a two year 100% manufacturer’s warranty covering workmanship and material for all units.

Any bidder failing to provide the required Warranties of FHWA Acceptance letter will be disqualified.

|  |  |  |  |
| --- | --- | --- | --- |
| SEPARATOR | 100% ROAD HAZARD Warranty for Separator, Reflectors and Mollies | Partial (60%) ROAD HAZARD Warranty for  Separator, Reflectors and Mollies | 100% Workmanship and Materials Warranty for all units |
| QWICK KURB® | 3 YEARS | YEARS 4 TO 5 | 2 YEARS |

1. **Construction.** Qwick Kurb shall be installed per manufactures instructions for Long Term Installation Manual
2. **Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay items:

**Pay Item Pay Unit**

\_Qwick Kurb, White……………. .................................................................................Each

SGJJR:AMR 2 of 2 01-24-17

**\_Qwick Kurb, White** will be measured and paid for at the contract unit price per each unit installed. The curb shall consist of section types L60, L61 and L62 with Uprights to be provided with a white post, white base and green reflective sheeting. The unit price shall be payment in full for furnishing all labor, equipment and material to furnish and install curbs as shown on the plans or as directed by the Engineer.