|  |  |  |
| --- | --- | --- |
|  | CITY OF DETROIT |  |
| SPECIAL PROVISION FOR  **BAND SIGN**  **(ON EXISTING LIGHT/UTILITY POLE)** |  |
| SGJJR:ESM | 1 of 1 | 01-24-17 |

1. **Description.** This work consists of furnishing materials necessary to attach signs onto existing light or utility poles and installing sign on existing poles as shown on the plans and as directed by the Engineer.
2. **Materials.** Furnish ½” stainless steel strap bands and buckles and heavy duty aluminum mounting plate with bolt and nut. Furnish tools and equipment as recommended by the manufacturer to install strap bands and mounting plate on exiting poles. Use equipment and materials from a single manufacturer throughout the entire project.
3. **Construction.** Strap bands, buckles, and mounting plates with bolts shall be secured to each existing pole. Signs shall be installed with minimum two mounting plates per sign per pole. Secure sign to mounting plate with bolts.
4. **Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay items:

**Pay Item Pay Unit**

\_Band, Sign (On Exist. Light/Utility Pole)....................................................................Each

**\_Band, Sign (On Exist. Light/Utility Pole)** will be measured and paid for at the contract unit price per each unit installed. The unit price shall be payment in full for furnishing all labor, equipment and material to furnish and install strap bands, buckles, mounting plates, bolts and nuts. Signs shall be measured and paid for under separate pay item.